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Heads up 1/8 mile all run on a .400 Pro tree

Car
· VW or Porsche door cars, convertibles, and Manx style buggies only.
· No dragsters, open frame buggies, or altered
· All vehicles must have proper safety equipment and driver’s license for E.T. run.
· All vehicles must have engine and transmission oil containment devices.
· All vehicles must have wheel to tire screws or bead locks.

Engine
· Rear Engine 4 cylinder Air-Cooled


Transmission
· No Automatics

Courtesy staging encouraged, double bulbs will be asked to back out by starter one time per race during eliminations, and second offense may be disqualified at starter’s discretion. Quickest winner of each round will have lane choice the following round.

