Race director will be: Dino Mendoza (626) 278-7825
Cruise Rules
At any time during the race the officials reserve to right to collect fuel samples that will be sent for testing. Violators will be banned for the year/season.
The Race Director will have the final call on all race rules and disputes. 
Street cruise the day of the race is MANDATORY!
· To participate in the cruise/race you must buy-in the day of the event, before cruise or in Real Street pits (At the discretion of the Race Director)
· No stops, Repairs or refueling during the street cruise.
· Breakdowns during the cruise will eliminate you from the race.
· Must show up with empty gas tank or pump the entire system before you refill at gas station where cruise starts. 
· Gas tanks will be sealed prior to cruise by race director (in the event that fuel is needed, only the race director can remove seal)
· Cars with aftermarket fittings for gas tank breather must be sealed at cruise along with the gas cap. 
· Entry fee must be submitted no later than the time of the street cruise or at the discretion of the Rase Director.
· No driver swaps! (same driver for cruise & race)
· Driver of the cruise and the race is awarded the points for the round (No Exceptions or Substitutions)



Engine and Vehicle Restrictions
· Weight for engine combinations as follows:
· Light 		(1738lbs= 82mm stroke X 94mm bore)
· Medium 	(1775lbs= 84mm stroke X 94 mm bore)
· Heavy 		(1825lbs= 86mm stroke X 94 mm bore)
· 91 Octane max (No E85)
· All factory style body parts are allowed as long they are bolted like stock body parts.
· NO Dzus buttons on outside body panels anywhere. 
· Package tray areas, firewall and the shell of the VW must not be cut out. 
· Must run with decklid on. No more than a 10in gap between decklid and body (Top or Bottom)
· Lexan/polycarbonate windows are permitted but must be mounted in stock rubber, no flush mount, no exceptions. 
· Carbon and fiberglass body parts are allowed but must be bolted on like stock.
· Minimum trimming in engine compartment and rear apron allowed.
· Min 2 seats required- must have front door panels (matching seats or a stock passenger seat)
· All Motor (carbureted only) 48 MM bore carburetor as max.
· No power adders
· No Fuel Injection
· No mixed fuels (No octane boosters or fuel additives)
· No fuel chillers (in vehicle)
· No vacuum pump.
· No roller camshaft
· No dry sumps (must be wet, stock or deep sump)
· No wheelie bars.
· No clutch management of any kind
· No spool/No electronic lockers
· STOCK VW dual-port intake stud location only! Manifold cannot be oversized (intake stud must remain 8 mm and in the stock location.)
· Functioning 4 wheel brakes required
· DOT approved tires required on all 4 wheels. 
·  235 60 15 max on the rear (cheaters, or street radials, front rollers okay)
· Engine cooling system and tins must always remain on the engine, fan belt could be removed (Stock shroud or 911 style allowed)
· No stingers (must run minimum 8” bullet style or 6” chambered muffler)
· Carburetor may have 48.0mm throttle plates with 44 mm venturi or smaller, Berg venturi is okay
· IDA, IDF, DRLA, replicas & copies are allowed. Mods are OK as long as they remain mechanical and have the required throttle plates and venturis. 
· Stock transmission location is required.
· IRS trailing arms, 1inch narrow allowed.
· No raise or narrowing of torsion housing allowed.
· Type 2 transmission allowed must be within 1 inch of stock location.
· 1-inch transmission raise is legal for Type 1 only.
· No E.T. trigger in front of the car. (front bumper, T-bar or no bumpers is OK)
· No chop tops, roof sectioning, channeling, or shortening of floor pan or body.
· Standard wheelbase, no scattered front wheels.

Race Day Rules

· Protest Rule: Should illegal activity (cheating) be suspected, a charge of $500 will be imposed to tear down motor.
· Cars can and will be inspected at any given time to ensure rules are followed.
· Registration and insurance required (will be verified at the buy in)
· Fuel will be checked for octane levels for finalist and #1 qualifier.
· 1/8 mile Heads Up
· Pro light “pro .004”
· Repairs during the race are allowed, as along as its policed by our class official and another Real Street Racer participant (no exceptions or will be disqualified)
· Must replace with similar part- not of higher performance.
· Timing and jets can be changed as needed.
· No oil changes permitted on premises or surrounding area the day of the race, no exceptions!
· No engine removal after the first qualifying round. No Exceptions. 
· $50 buy in on race day, pay outs will be determined by the number of entries and the available sponsorship money.
· Winner and runner up’s engines will be pumped at each race to ensure the integrity of the class.
· All vehicles must roll across the scales at time of tech with every pass. No Scales = instant Disqualification
· All cars must Scale and meet weight restrictions. Lite cars will result in instant disqualification.
· One warning during qualifying if the car doesn't have a roll cage if the car runs an illegal number during eliminations instant disqualification.
· Swapping wheels between cruise and race is ok as long as the tires on the track are DOT approved.
· Finalist will have to drain their entire fuel system. Officials will provide 2.5 gallons for each contender of the final round
· Race will be based on a 16-car ladder. In the event that the car minimum is not met, we will run the appropriate ladder from the fastest qualifiers.
· The race director will have the final say in any dispute. The ruling will stand. 

All vehicles must meet NHRA safety requirements per E.T. and MPH ran PLEASE PARK CLOSE TOGETHER TO FACILITATE THE PROGRAM!!!!
Be respectful to the Race Director, Each other, and the Track Officials “talking trash” on Facebook or elsewhere is not going to make you quicker or faster on Race Day -we are encouraging a peaceful, positive racing family atmosphere. Thank you!
