PRO OUTLAW RULES

[bookmark: _GoBack]Heads up 1/8 mile all run on a .400 Pro tree

Car
· VW or Porsche door cars, convertibles, and Manx style buggies
· No dragsters, open frame buggies, or altered
· All vehicles must have a windshield and proper safety equipment and driver’s license for E.T. run.
· All vehicles must have engine and transmission oil containment devices.
· All vehicles must have wheel to tire screws or bead locks.
· Minimum Weight 1,500lbs car and driver

Engine
· Rear Engine Type 1 Air-Cooled
· Limited to 1 Power Adder
· Turbo & Nitrous Cars  - 94mm Max Bore, No Intercooler
· N/A Cars - No limit on Engine Size
· No Nitro allowed

Transmission
· No sequential transmissions. 
· All vehicles must be manually shifted by hand, no paddle, ECU controlled, or Co2 shifters.
· No leaving on a button.
· Driver must lift a foot off of a mechanical clutch pedal to leave starting line.
· Ignition interrupt/clutch less shifting allowed but must be manually shifted by hand.
· No traction control

Courtesy staging encouraged, double bulbs will be asked to back out by starter one time per race during eliminations, and second offense may be disqualified at starter’s discretion. Quickest winner of each round will have lane choice the following round. 


